

SECTION 12 56 00 – INSTITUTIONAL FURNITURE

DINING COMMONS – ELEMENTARY SCHOOL

SPECIFIER NOTE: THESE SPECIFICATIONS WERE CURRENT AT THE TIME OF PUBLICATION BUT ARE SUBJECT TO CHANGE AT ANY TIME WITHOUT NOTICE. PLEASE CONFIRM THE ACCURACY OF THESE SPECIFICATIONS WITH THE MANUFACTURER AND/OR DISTRIBUTOR PRIOR TO CONSTRUCTION OR INSTALLATION.

GUIDE SPECIFICATIONS:

THIS GUIDE SPECIFICATION IS WRITTEN ACCORDING TO THE CONSTRUCTION SPECIFICATIONS INSTITUTE (CSI) FORMATS, INCLUDING MASTERFORMAT®, SECTIONFORMAT™, AND PAGEFORMAT™.

CAREFULLY REVIEW AND EDIT THIS SECTION TO MEET THE REQUIREMENTS OF THE PROJECT, LOCAL BUILDING CODE AND AUTHORITIES HAVING JURISDICTION. COORDINATE THIS SECTION WITH OTHER SPECIFICATION SECTIONS AND DRAWINGS.

DELETE ALL "SPECIFIER NOTES" WHEN EDITING THIS SECTION.

# GENERAL

## CONDITIONS AND REQUIREMENTS

### The General Conditions, Supplementary Conditions, and Division 01 – General Requirements apply.

## SECTION INCLUDES

## Mobile Bench Tables.

## Mobile Stool Tables.

## Mobile Stool and Bench Tables.

## All-In-One Mobile Convertible Benches.

## Mobile Convertible Benches.

## All-In-One Mobile Convertible Benches with Tables – Packages.

## Buddy Bench.

## Heavy-Duty Receptacles.

## Heavy-Duty Condiment Cabinets.

## QUALITY ASSURANCE

## Elementary school dining commons product manufacturer shall have a minimum of 65 years of experience.

## REFERENCES

### American National Standards Institute (ANSI):

### ANSI Certified.

### Business and Institutional Furniture Manufacturers Association (BIFMA):

### BIFMA Certified.

## SUBMITTALS

### Product Data:

#### Submit manufacturer's printed product literature, specifications, warranty statement, and data sheet.

## WARRANTY

### Manufacturer’s Warranty: Provide manufacturer’s standard limited warranty in effect at the date of purchase.

# PRODUCTS

## MANUFACTURERS

### Specified Manufacturer: AmTab, 600 Eagle Drive, Bensenville, IL. Telephone: 630-301-7600. Email: info@amtab.com. Web: [www.AmTab.com](http://www.AmTab.com).

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SPECIFIER NOTES: DELETE ONE OF THE FOLLOWING TWO PARAGRAPHS.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

### Substitutions: Not Permitted.

## ELEMENTARY SCHOOL DINING COMMONS

### AmTab is a full-service branding, interior design, manufacturing, and installation firm. AmTab creates modern, popular, and fun K-12 Learning Environments, specializing in Dining Commons and Food Courts with Furniture, Signage, Graphics, and Décor. AmTab builds strong partnerships with clients that last a lifetime. The products in this specification are designed for use in the dining commons of elementary schools. These products include mobile bench tables, mobile stool tables, mobile stool and bench tables, benches, receptacles, and condiment cabinets. AmTab products are ANSI and BIFMA certified.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SPECIFIER NOTES: DELETE PRODUCTS AND OPTIONS NOT REQUIRED FOR THIS PROJECT. OPTIONS WITHIN PRODUCTS ARE INDICATED BY SQUARE BRACKETS.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

### AmTab Product Options:

#### Mix and Match Standard Table Top and Bench Laminates: [Wilsonart Standard Laminates], [Formica Standard Laminates], [Pionite Standard Laminates], [Nevamar Standard Laminates], [Arborite Standard Laminates], [Laminart Standard Laminates], or [Egger Standard Laminates].

#### Mix and Match Upgrade Premium Table Top Laminates: [Wilsonart Premium Laminates], [Formica Premium Laminates], [Pionite Premium Laminates], [Nevamar Premium Laminates], [Arborite Premium Laminates], [Laminart Premium Laminates], or [Egger Premium Laminates].

#### Mix and Match Standard T-Molding Table Top and Bench Edge Colors: [Black], [Brown], [Gray], [Beige], [Navy Blue], [Red], [Burgundy], [Light Green], [Yellow], [Blue], [Hunter Green], [Orange], [Purple], [Green], [Light Blue], [Gold], or [Aqua Teal].

#### Mix and Match Upgrade Dyna-Rock Table Top and Bench Edge Colors: [Black], [Brown], [Gray], [Beige], [Navy Blue], [Red], [Burgundy], [Light Green], [Yellow], [Blue], [Hunter Green], [Orange], [Purple], [Green], [Light Blue], [Gold], [Pink], or [Aqua Teal].

#### Standard Metal Finishes: [Titanium], [Champagne], [Charcoal], [Black], [Brown], [Gray], [Beige], or [White].

#### Mix and Match Upgrade Wheel Colors: [Black], [Brown], [Gray], [Beige], [Navy Blue], [Red], [Burgundy], [Light Green], [Yellow], [Blue], [Hunter Green], [Orange], [Purple], [Green], [Light Blue], [Gold], or [Aqua Teal].

#### Deluxe Stool with Two Colors: Patented stool design and square steel tube column available in [Round] or Rectangle].

#### Mix and Match Standard Stool Top and Stool Bottom Colors: [Black], [Brown], [Gray], [Beige], [Navy Blue], [Red], [Burgundy], [Light Green], [Yellow], [Blue], [Hunter Green], [Orange], [Purple], [Green], [Light Blue], [Gold], [White], [Pink], [Silver], or [Aqua Teal].

#### Mix and Match Upgrade Custom Logo Table Top and Bench: Contact the manufacturer for custom logo tops.

#### Upgrade Metal Finish: Chrome.

#### Upgrade Core: Plywood.

#### Upgrade ADA: [ADA Accessible], [1 ADA accessible spot] or [2 ADA accessible spots].

## MOBILE BENCH TABLES

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SPECIFIER NOTES: DELETE PRODUCTS AND OPTIONS NOT REQUIRED FOR THIS PROJECT. OPTIONS WITHIN PRODUCTS ARE INDICATED BY SQUARE BRACKETS.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

### Mobile Bench Tables

#### Mobile Bench Tables – Rectangle MBT08

#### Features:

#### Cleaning Position: Intermediate locking position allows for easy cleaning, set up, and reset up.

#### Multiple Entrances: E-Z Free™ multiple entrances for easy access and comfort.

#### Opening and Closing: High Powered High Speed™ gas cylinders for long-lasting opening and closing functions.

#### Locking: E-Z Autolock™ automatically locks the table when folded and opens from either side.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Casters: Heavy-duty casters to ensure quality and durability.

#### Physical Characteristics:

#### Shape: Rectangle.

#### Table:

#### Width: 30 inches (76 centimeters).

#### Length: 8 feet 1 inch (246 centimeters).

#### Table and Bench Height: [29 – 17 inches (74 centimeters – 43 centimeters)] or [27 –17 inches (69 centimeters – 43 centimeters)].

#### Seats: 8 to 12.

#### Mobile Bench Tables – Rectangle MBT10

#### Features:

#### Cleaning Position: Intermediate locking position allows for easy cleaning, set up, and reset up.

#### Multiple Entrances: E-Z Free™ multiple entrances for easy access and comfort.

#### Opening and Closing: High Powered High Speed™ gas cylinders for long-lasting opening and closing functions.

#### Locking: E-Z Autolock™ automatically locks the table when folded and opens from either side.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Casters: Heavy-duty casters to ensure quality and durability.

#### Physical Characteristics:

#### Shape: Rectangle.

#### Table :

#### Width: 30 inches (76 centimeters).

#### Length: 10 feet 1 inch (307 centimeters).

#### Table and Bench Height: [29 – 17 inches (74 centimeters – 43 centimeters)] or [27 –17 inches (69 centimeters – 43 centimeters)].

#### Seats: 10 to 14.

#### Mobile Bench Tables – Rectangle MBT12

#### Features:

#### Cleaning Position: Intermediate locking position allows for easy cleaning, set up, and reset up.

#### Multiple Entrances: E-Z Free™ multiple entrances for easy access and comfort.

#### Opening and Closing: High Powered High Speed™ gas cylinders for long-lasting opening and closing functions.

#### Locking: E-Z Autolock™ automatically locks the table when folded and opens from either side.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Casters: Heavy-duty casters to ensure quality and durability.

#### Physical Characteristics:

#### Shape: Rectangle.

#### Table:

#### Width: 30 inches (76 centimeters).

#### Length: 12 feet 1 inch (368 centimeters).

#### Table and Bench Height: [29 – 17 inches (74 centimeters – 43 centimeters)] or [27 –15 inches (69 centimeters – 38 centimeters)].

#### Seats: 12 to 16.

#### Mobile Bench Tables – Wave MBWT10

#### Features:

#### Cleaning Position: Intermediate locking position allows for easy cleaning, set up, and reset up.

#### Multiple Entrances: E-Z Free™ multiple entrances for easy access and comfort.

#### Opening and Closing: High Powered High Speed™ gas cylinders for long-lasting opening and closing functions.

#### Locking: E-Z Autolock™ automatically locks the table when folded and opens from either side.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Casters: Heavy-duty casters to ensure quality and durability.

#### Physical Characteristics:

#### Shape: Wave.

#### Table:

#### Width: 35 inches (89 centimeters).

#### Length: 10 feet 1 inch (307 centimeters).

#### Table and Bench Height: [29 – 17 inches (74 centimeters – 43 centimeters)] or [27 –17 inches (69 centimeters – 43 centimeters)].

#### Seats: 10 to 14.

#### Mobile Bench Tables – Wave MBWT12

#### Features:

#### Cleaning Position: Intermediate locking position allows for easy cleaning, set up, and reset up.

#### Multiple Entrances: E-Z Free™ multiple entrances for easy access and comfort.

#### Opening and Closing: High Powered High Speed™ gas cylinders for long-lasting opening and closing functions.

#### Locking: E-Z Autolock™ automatically locks the table when folded and opens from either side.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Casters: Heavy-duty casters to ensure quality and durability.

#### Physical Characteristics:

#### Shape: Wave.

#### Table:

#### Width: 35 inches (89 centimeters).

#### Length: 12 feet 1 inch (368 centimeters).

#### Table and Bench Height: [29 – 17 inches (74 centimeters – 43 centimeters)] or [27 –15 inches (69 centimeters – 38 centimeters)].

#### Seats: 12 to 16.

#### Mobile Bench Tables – Elliptical MBE10

#### Features:

#### Cleaning Position: Intermediate locking position allows for easy cleaning, set up, and reset up.

#### Locking: E-Z Autolock™ automatically locks the table when folded and opens from either side.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Casters: Heavy-duty casters to ensure quality and durability.

#### Physical Characteristics:

#### Shape: Elliptical.

#### Table:

#### Width: 46 inches (117 centimeters).

#### Length: 10 feet 1 inch (307 centimeters).

#### Table and Bench Height: [29 – 17 inches (74 centimeters – 43 centimeters)] or [[27 –15 inches (69 centimeters – 38 centimeters)].

#### Seats: 10 to 14.

#### Mobile Bench Tables – Round MBR604

#### Features:

#### Cleaning Position: Intermediate locking position allows for easy cleaning, set up, and reset up.

#### Locking: E-Z Autolock™ automatically locks the table when folded and opens from either side.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Casters: Heavy-duty casters to ensure quality and durability.

#### Physical Characteristics:

#### Shape: Round.

#### Table:

#### Diameter: 60 inches (152 centimeters).

#### Table and Bench Height: [29 – 17 inches (74 centimeters – 43 centimeters)], [27 –15 inches (69 centimeters – 38 centimeters)], or [25 – 13 inches (64 – 33 centimeters)].

#### Seats: 8.

#### Mobile Bench Tables – Octagon MBROC604

#### Features:

#### Cleaning Position: Intermediate locking position allows for easy cleaning, set up, and reset up.

#### Locking: E-Z Autolock™ automatically locks the table when folded and opens from either side.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Casters: Heavy-duty casters to ensure quality and durability.

#### Physical Characteristics:

#### Shape: Octagon.

#### Table:

#### Diameter: 60 inches (152 centimeters).

#### Table and Bench Height: [29 – 17 inches (74 centimeters – 43 centimeters)], [27 –15 inches (69 centimeters – 38 centimeters)], or [25 – 13 inches (64 – 33 centimeters)].

#### Seats: 8.

## MOBILE STOOL TABLES

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SPECIFIER NOTES: DELETE PRODUCTS AND OPTIONS NOT REQUIRED FOR THIS PROJECT. OPTIONS WITHIN PRODUCTS ARE INDICATED BY SQUARE BRACKETS.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

### Mobile Stool Tables

#### Mobile Stool Tables – Round MSR608

#### Features:

#### Cleaning Position: Intermediate locking position allows for easy cleaning, set up, and reset up.

#### Opening and Closing: High Powered High Speed™ gas cylinders for long-lasting opening and closing functions.

#### Locking: E-Z Autolock™ automatically locks the table when folded and opens from either side.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Physical Characteristics:

#### Shape: Round.

#### Table:

#### Diameter: 60 inches (152 centimeters).

#### Table and Bench Height: [29 – 17 inches (74 centimeters – 43 centimeters)], [27 –15 inches (69 centimeters – 38 centimeters)], or [25 – 13 inches (64 – 33 centimeters)].

#### Stools: 8.

#### Mobile Stool Tables – Octagon MSOC608

#### Features:

#### Cleaning Position: Intermediate locking position allows for easy cleaning, set up, and reset up.

#### Opening and Closing: High Powered High Speed™ gas cylinders for long-lasting opening and closing functions.

#### Locking: E-Z Autolock™ automatically locks the table when folded and opens from either side.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Physical Characteristics:

#### Shape: Octagon.

#### Table:

#### Width: 60 inches (152 centimeters).

#### Table and Bench Height: [29 – 17 inches (74 centimeters – 43 centimeters)], [27 –15 inches (69 centimeters – 38 centimeters)], or [25 – 13 inches (64 – 33 centimeters)].

#### Stool Size: 14 inches (36 centimeters).

#### Seats: 8.

#### Mobile Stool Tables – Elliptical MSE610

#### Features:

#### Cleaning Position: Intermediate locking position allows for easy cleaning, set up, and reset up.

#### Opening and Closing: High Powered High Speed™ gas cylinders for long-lasting opening and closing functions.

#### Locking: E-Z Autolock™ automatically locks the table when folded and opens from either side.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Physical Characteristics:

#### Shape: Elliptical.

#### Table:

#### Width: 54 inches (137 centimeters).

#### Length: 6 feet 1 inches (185 centimeters).

#### Table and Bench Height: [29 – 17 inches (74 centimeters – 43 centimeters)], [27 –15 inches (69 centimeters – 38 centimeters)], or [25 – 13 inches (64 – 33 centimeters)].

#### Stool Size: 14 inches (36 centimeters).

#### Stools: 10.

#### Mobile Stool Tables – Elliptical MSE1012

#### Features:

#### Cleaning Position: Intermediate locking position allows for easy cleaning, set up, and reset up.

#### Opening and Closing: High Powered High Speed™ gas cylinders for long-lasting opening and closing functions.

#### Locking: E-Z Autolock™ automatically locks the table when folded and opens from either side.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Physical Characteristics:

#### Shape: Elliptical

#### Table:

#### Width: 46 inches (117 centimeters).

#### Length: 10 feet 1 inch (307 centimeters).

#### Table and Bench Height: [29 – 17 inches (74 centimeters – 43 centimeters)], [27 –15 inches (69 centimeters – 38 centimeters)], or [25 – 13 inches (64 – 33 centimeters)].

#### Stool Size: 14 inches (36 centimeters).

#### Stools: 12.

#### Mobile Stool Tables – Rectangle MST44

#### Features:

#### Cleaning Position: Intermediate locking position allows for easy cleaning, set up, and reset up.

#### Opening and Closing: High Powered High Speed™ gas cylinders for long-lasting opening and closing functions.

#### Locking: E-Z Autolock™ automatically locks the table when folded and opens from either side.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Physical Characteristics:

#### Shape: Rectangle.

#### Table:

#### Width: 30 inches (76 centimeters).

#### Length: 4 feet (122 centimeters).

#### Table and Bench Height: [29 – 17 inches (74 centimeters – 43 centimeters)], [27 –15 inches (69 centimeters – 38 centimeters)], or [25 – 13 inches (64 – 33 centimeters)].

#### Stool Size: 14 inches (36 centimeters).

#### Stools: 4.

#### Mobile Stool Tables – Rectangle MST88

#### Features:

#### Cleaning Position: Intermediate locking position allows for easy cleaning, set up, and reset up.

#### Opening and Closing: High Powered High Speed™ gas cylinders for long-lasting opening and closing functions.

#### Locking: E-Z Autolock™ automatically locks the table when folded and opens from either side.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Physical Characteristics:

#### Shape: Rectangle.

#### Table:

#### Width: 30 inches (76 centimeters).

#### Length: 8 feet 1 inch (246 centimeters).

#### Table and Bench Height: [29 – 17 inches (74 centimeters – 43 centimeters)], [27 –15 inches (69 centimeters – 38 centimeters)], or [25 – 13 inches (64 – 33 centimeters)].

#### Stool Size: 14 inches (36 centimeters).

#### Stools: 8.

#### Mobile Stool Tables – Rectangle MST1012

#### Features:

#### Cleaning Position: Intermediate locking position allows for easy cleaning, set up, and reset up.

#### Opening and Closing: High Powered High Speed™ gas cylinders for long-lasting opening and closing functions.

#### Locking: E-Z Autolock™ automatically locks the table when folded and opens from either side.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Physical Characteristics:

#### Shape: Rectangle.

#### Table:

#### Width: 30 inches (76 centimeters).

#### Length: 10 feet 1 inch (307 centimeters).

#### Table and Bench Height: [29 – 17 inches (74 centimeters – 43 centimeters)], [27 –15 inches (69 centimeters – 38 centimeters)], or [25 – 13 inches (64 – 33 centimeters)].

#### Stool Size: 14 inches (36 centimeters).

#### Stools: 12.

#### Mobile Stool Tables – Rectangle MST1212

#### Features:

#### Cleaning Position: Intermediate locking position allows for easy cleaning, set up, and reset up.

#### Opening and Closing: High Powered High Speed™ gas cylinders for long-lasting opening and closing functions.

#### Locking: E-Z Autolock™ automatically locks the table when folded and opens from either side.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Physical Characteristics:

#### Shape: Rectangle.

#### Table:

#### Width: 30 inches (76 centimeters).

#### Length: 12 feet 1 inch (368 centimeters).

#### Table and Bench Height: [29 – 17 inches (74 centimeters – 43 centimeters)], [27 –15 inches (69 centimeters – 38 centimeters)], or [25 – 13 inches (64 – 33 centimeters)].

#### Stool Size: 14 inches (36 centimeters).

#### Stools: 12.

#### Mobile Stool Tables – Rectangle MST1216

#### Features:

#### Cleaning Position: Intermediate locking position allows for easy cleaning, set up, and reset up.

#### Opening and Closing: High Powered High Speed™ gas cylinders for long-lasting opening and closing functions.

#### Locking: E-Z Autolock™ automatically locks the table when folded and opens from either side.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Physical Characteristics:

#### Shape: Rectangle.

#### Table:

#### Width: 30 inches (76 centimeters).

#### Length: 12 feet 1 inch (368 centimeters).

#### Table and Bench Height: [29 – 17 inches (74 centimeters – 43 centimeters)], [27 –15 inches (69 centimeters – 38 centimeters)], or [25 – 13 inches (64 – 33 centimeters)].

#### Stool Size: 14 inches (36 centimeters).

#### Stools: 16.

#### Mobile Stool Tables – Wave MSWT1012

#### Features:

#### Cleaning Position: Intermediate locking position allows for easy cleaning, set up, and reset up.

#### Opening and Closing: High Powered High Speed™ gas cylinders for long-lasting opening and closing functions.

#### Locking: E-Z Autolock™ automatically locks the table when folded and opens from either side.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Physical Characteristics:

#### Shape: Wave.

#### Table:

#### Width: 35 inches (89 centimeters).

#### Length: 10 feet 1 inch (307 centimeters).

#### Table and Bench Height: [29 – 17 inches (74 centimeters – 43 centimeters)], [27 –15 inches (69 centimeters – 38 centimeters)], or [25 – 13 inches (64 – 33 centimeters)].

#### Stool Size: 14 inches (36 centimeters).

#### Stools: 12.

#### Mobile Stool Tables – Wave MSWT1212

#### Features:

#### Cleaning Position: Intermediate locking position allows for easy cleaning, set up, and reset up.

#### Opening and Closing: High Powered High Speed™ gas cylinders for long-lasting opening and closing functions.

#### Locking: E-Z Autolock™ automatically locks the table when folded and opens from either side.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Physical Characteristics:

#### Shape: Wave.

#### Table:

#### Width: 35 inches (89 centimeters).

#### Length: 12 feet 1 inch (368 centimeters).

#### Table and Bench Height: [29 – 17 inches (74 centimeters – 43 centimeters)], [27 –15 inches (69 centimeters – 38 centimeters)], or [25 – 13 inches (64 – 33 centimeters)].

#### Stool Size: 14 inches (36 centimeters).

#### Stools: 12.

#### Mobile Stool Tables – Wave MSWT1216

#### Features:

#### Cleaning Position: Intermediate locking position allows for easy cleaning, set up, and reset up.

#### Opening and Closing: High Powered High Speed™ gas cylinders for long-lasting opening and closing functions.

#### Locking: E-Z Autolock™ automatically locks the table when folded and opens from either side.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Physical Characteristics:

#### Shape: Wave.

#### Table:

#### Width: 35 inches (89 centimeters).

#### Length: 12 feet 1 inch (368 centimeters).

#### Table and Bench Height: [29 – 17 inches (74 centimeters – 43 centimeters)], [27 –15 inches (69 centimeters – 38 centimeters)], or [25 – 13 inches (64 – 33 centimeters)].

#### Stool Size: 14 inches (36 centimeters).

#### Stools: 16.

## MOBILE STOOL AND BENCH TABLES

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SPECIFIER NOTES: DELETE PRODUCTS AND OPTIONS NOT REQUIRED FOR THIS PROJECT. OPTIONS WITHIN PRODUCTS ARE INDICATED BY SQUARE BRACKETS.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

### Mobile Stool and Bench Tables

#### Mobile Stool and Bench Tables – Round MSBR6042

#### Features:

#### Cleaning Position: Intermediate locking position allows for easy cleaning, set up, and reset up.

#### Opening and Closing: High Powered High Speed™ gas cylinders for long-lasting opening and closing functions.

#### Locking: E-Z Autolock™ automatically locks the table when folded and opens from either side.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Physical Characteristics:

#### Shape: Round.

#### Table Diameter: 60 inches (152 centimeters).

#### Table and Bench/Stool Height: [29 – 17 inches (74 centimeters – 43 centimeters)], [27 –15 inches (69 centimeters – 38 centimeters)], or [25 – 13 inches (64 – 33 centimeters)].

#### Stool Size: 14 inches (36 centimeters).

#### Stools: 4.

#### Benches: 2.

#### Mobile Stool and Bench Tables – Wave MSBWT1062

#### Features:

#### Cleaning Position: Intermediate locking position allows for easy cleaning, set up, and reset up.

#### Opening and Closing: High Powered High Speed™ gas cylinders for long-lasting opening and closing functions.

#### Locking: E-Z Autolock™ automatically locks the table when folded and opens from either side.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Physical Characteristics:

#### Shape: Wave.

#### Table:

#### Width: 35 inches (89 centimeters).

#### Length: 10 feet 1 inch (307 centimeters).

#### Table and Bench/Stool Height: [29 – 17 inches (74 centimeters – 43 centimeters)] or [27 –17 inches (69 centimeters – 43 centimeters)].

#### Stool Size: 14 inches (36 centimeters).

#### Stools: 6.

#### Benches: 2.

#### Mobile Stool and Bench Tables – Wave MSBWT1262

#### Features:

#### Cleaning Position: Intermediate locking position allows for easy cleaning, set up, and reset up.

#### Opening and Closing: High Powered High Speed™ gas cylinders for long-lasting opening and closing functions.

#### Locking: E-Z Autolock™ automatically locks the table when folded and opens from either side.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Physical Characteristics:

#### Shape: Wave.

#### Table:

#### Width: 35 inches (89 centimeters).

#### Length: 12 feet 1 inch (368 centimeters).

#### Table and Bench/Stool Height: [29 – 17 inches (74 centimeters – 43 centimeters)] or [27 –15 inches (69 centimeters – 38 centimeters)],

#### Stool Size: 14 inches (36 centimeters).

#### Stools: 6.

#### Benches: 2.

#### Mobile Stool and Bench Tables – Elliptical MSBE1062

#### Features:

#### Cleaning Position: Intermediate locking position allows for easy cleaning, set up, and reset up.

#### Opening and Closing: High Powered High Speed™ gas cylinders for long-lasting opening and closing functions.

#### Locking: E-Z Autolock™ automatically locks the table when folded and opens from either side.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Physical Characteristics:

#### Shape: Elliptical.

#### Table:

#### Width: 35 inches (89 centimeters).

#### Length: 10 feet 1 inch (307 centimeters).

#### Table and Bench/Stool Height: [29 – 17 inches (74 centimeters – 43 centimeters)] or [27 –17

#### Stool Size: 14 inches (36 centimeters).

#### Stools: 6.

#### Benches: 2.

## ALL-IN-ONE MOBILE CONVERTIBLE BENCHES

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SPECIFIER NOTES: DELETE PRODUCTS AND OPTIONS NOT REQUIRED FOR THIS PROJECT. OPTIONS WITHIN PRODUCTS ARE INDICATED BY SQUARE BRACKETS.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

### All-In-One Mobile Convertible Benches

#### Features:

#### Safety: Built-in safety feature prevents fingers from being pinched when folding table.

#### Frame: Heavy duty 14 guage steel frame with gussets.

#### Coupling: E-Z Coupling Device for table-to-table coupling on all standard models.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Legs: Top support legs to provide extra support, strength and stability to the table top.

#### Caster Beam: The shortest caster beam for the best solution for adding seating capacity and safety in the industry.

#### Casters: Heavy-duty casters to ensure quality and durability.

#### Storage: Compacting nesting in storage with all-in-one design for easy set up and compact storage.

#### All-In-One Mobile Convertible Bench ACB4

#### Physical Characteristics:

#### Table:

#### Width: 29 inches (89 centimeters).

#### Length: 48 inches (307 centimeters).

#### Table and Bench Height: [29 – 17 inches (74 centimeters – 43 centimeters)], or [27 –15 inches (69 centimeters – 38 centimeters)].

#### Seats: 2 to 3.

#### All-In-One Mobile Convertible Bench ACB5

#### Physical Characteristics:

#### Table:

#### Width: 29 inches (89 centimeters).

#### Length: 60 inches (152 centimeters).

#### Table and Bench Height: [29 – 17 inches (74 centimeters – 43 centimeters)], or [27 –15 inches (69 centimeters – 38 centimeters)].

#### Seats: 2 to 3.

#### All-In-One Mobile Convertible Bench ACB6

#### Physical Characteristics:

#### Table:

#### Width: 29 inches (89 centimeters).

#### Length: 72 inches (183 centimeters).

#### Table and Bench Height: [29 – 17 inches (74 centimeters – 43 centimeters)], or [27 –15 inches (69 centimeters – 38 centimeters)].

#### Seats: 3 to 4.

#### All-In-One Mobile Convertible Bench ACB7

#### Physical Characteristics:

#### Table:

#### Width: 29 inches (89 centimeters).

#### Length: 84 inches (213 centimeters).

#### Table and Bench Height: [29 – 17 inches (74 centimeters – 43 centimeters)], or [27 –15 inches (69 centimeters – 38 centimeters)].

#### Seats: 4 to 5.

#### All-In-One Mobile Convertible Bench ACB8

#### Physical Characteristics:

#### Table:

#### Width: 29 inches (89 centimeters).

#### Length: 96 inches (244 centimeters).

#### Table and Bench Height: [29 – 17 inches (74 centimeters – 43 centimeters)], or [27 –15 inches (69 centimeters – 38 centimeters)].

#### Seats: 4 to 6.

## MOBILE CONVERTIBLE BENCHES

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SPECIFIER NOTES: DELETE PRODUCTS AND OPTIONS NOT REQUIRED FOR THIS PROJECT. OPTIONS WITHIN PRODUCTS ARE INDICATED BY SQUARE BRACKETS.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

### Mobile Convertible Benches

#### Features:

#### Safety: Built-in safety feature prevents fingers from being pinched when folding table.

#### Frame: Heavy duty 14 guage steel frame with gussets.

#### Coupling: E-Z Coupling Device for table-to-table coupling on all standard models.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Mobile Convertible Bench MCB4

#### Physical Characteristics:

#### Table:

#### Width: 29 inches (89 centimeters).

#### Length: 48 inches (307 centimeters).

#### Table and Bench/Stool Height: [29 – 17 inches (74 centimeters – 43 centimeters)], or [27 –15 inches (69 centimeters – 38 centimeters)].

#### Seats: 2 to 3.

#### Mobile Convertible Bench MCB5

#### Physical Characteristics:

#### Table:

#### Width: 29 inches (89 centimeters).

#### Length: 60 inches (152 centimeters).

#### Table and Bench/Stool Height: [29 – 17 inches (74 centimeters – 43 centimeters)], or [27 –15 inches (69 centimeters – 38 centimeters)].

#### Seats: 2 to 3.

#### Mobile Convertible Bench MCB6

#### Physical Characteristics:

#### Table:

#### Width: 29 inches (89 centimeters).

#### Length: 72 inches (183 centimeters).

#### Table and Bench/Stool Height: [29 – 17 inches (74 centimeters – 43 centimeters)], or [27 –15 inches (69 centimeters – 38 centimeters)].

#### Seats: 3 to 4.

#### Mobile Convertible Bench MCB7

#### Physical Characteristics:

#### Table:

#### Width: 29 inches (89 centimeters).

#### Length: 84 inches (213 centimeters).

#### Table and Bench/Stool Height: [29 – 17 inches (74 centimeters – 43 centimeters)], or [27 –15 inches (69 centimeters – 38 centimeters)].

#### Seats: 4 to 5.

#### Mobile Convertible Bench MCB8

#### Physical Characteristics:

#### Table:

#### Width: 29 inches (89 centimeters).

#### Length: 96 inches (244 centimeters).

#### Table and Bench/Stool Height: [29 – 17 inches (74 centimeters – 43 centimeters)], or [27 –15 inches (69 centimeters – 38 centimeters)].

#### Seats: 4 to 6.

## ALL-IN-ONE MOBILE CONVERTIBLE BENCHES WITH TABLES – PACKAGES

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SPECIFIER NOTES: DELETE PRODUCTS AND OPTIONS NOT REQUIRED FOR THIS PROJECT. OPTIONS WITHIN PRODUCTS ARE INDICATED BY SQUARE BRACKETS.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

### All-In-One Mobile Convertible Benches with Table - Package

#### Features:

#### Safety: Built-in safety feature prevents fingers from being pinched when folding table.

#### Frame: Heavy duty 14 guage steel frame with gussets.

#### Coupling: E-Z Coupling Device for table-to-table coupling on all standard models.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Legs: Top support legs to provide extra support, strength and stability to the table top.

#### Caster Beam: The shortest caster beam for the best solution for adding seating capacity and safety in the industry.

#### Casters: Heavy-duty casters to ensure quality and durability.

#### Storage: Compacting nesting in storage with all-in-one design for easy set up and compact storage.

#### All-In-One Mobile Convertible Benches with Table ACBP244

#### Physical Characteristics:

#### Shape: Rectangle.

#### Table:

#### Width: 83 inches (211 centimeters).

#### Length: 48 inches (122 centimeters).

#### Height: 38 inches (97 centimeters).

#### Seats: 4 to 6.

#### All-In-One Mobile Convertible Benches with Table ACBP245

#### Physical Characteristics:

#### Shape: Rectangle.

#### Table:

#### Width: 83 inches (211 centimeters).

#### Length: 60 inches (152 centimeters).

#### Height: 38 inches (97 centimeters).

#### Seats: 6 to 8.

#### All-In-One Mobile Convertible Benches with Table ACBP304

#### Physical Characteristics:

#### Shape: Rectangle.

#### Table:

#### Width: 90 inches (229 centimeters).

#### Length: 48 inches (122 centimeters).

#### Height: 38 inches (97 centimeters).

#### Seats: 4 to 6.

#### All-In-One Mobile Convertible Benches with Table ACBP305

#### Physical Characteristics:

#### Shape: Rectangle.

#### Table:

#### Width: 90 inches (229 centimeters).

#### Length: 60 inches (152 centimeters).

#### Height: 38 inches (97 centimeters).

#### Seats: 6 to 8.

## BUDDY BENCH

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SPECIFIER NOTES: DELETE PRODUCTS AND OPTIONS NOT REQUIRED FOR THIS PROJECT. OPTIONS WITHIN PRODUCTS ARE INDICATED BY SQUARE BRACKETS.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

### Description: The AmTab Buddy Bench is the perfect way for students to be comfortable and safe while at school. The Buddy Bench can be fully customized to meet your needs. This bench ushers in a positive environment that helps prevent bullying and eliminates loneliness and fosters friendship in school

### Physical Characteristics

#### Features:

#### Safety: Built-in safety feature prevents fingers from being pinched when folding table.

#### Frame: Heavy duty 14 guage steel frame with gussets.

#### Coupling: E-Z Coupling Device for table-to-table coupling on all standard models.

#### Glides: Dynagrip™ custom glides are extra wide high impact non-marking load-bearing glides for floor safety.

#### Legs: Top support legs to provide extra support, strength and stability to the table top.

#### Caster Beam: The shortest caster beam for the best solution for adding seating capacity and safety in the industry.

#### Casters: Heavy-duty casters to ensure quality and durability.

#### Storage: Compacting nesting in storage with all-in-one design for easy set up and compact storage.

#### Bench Dimensions:

#### Model: BUDDYBENCH.

#### Table:

#### Width: 29 inches (74 centimeters).

#### Length: 96 inches (244 centimeters).

#### Height: 38 inches (97 centimeters).

#### Table and Bench Height: [29 – 17 inches (74 centimeters – 43 centimeters)], or [27 –15 inches (69 centimeters – 38 centimeters)].

#### Seats: 6 to 8.

## HEAVY-DUTY RECEPTACLES

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SPECIFIER NOTES: DELETE PRODUCTS AND OPTIONS NOT REQUIRED FOR THIS PROJECT. OPTIONS WITHIN PRODUCTS ARE INDICATED BY SQUARE BRACKETS.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

### Heavy-Duty Receptacles – Recycling and Waste

#### Product Options:

#### Mix and Match Upgrade Custom Logo for Front or Sides: Contact the manufacturer for custom logo tops.

#### Heavy-Duty Receptacle – Recycling – HDRR32

#### Physical Characteristics:

#### Width: 27 inches (69 centimeters).

#### Length: 27 inches (69 centimeters).

#### Height: 46 inches (117 centimeters).

#### Capacity: 32 gallons (121 liters).

#### Heavy-Duty Receptacle – Recycling – HDRR44

#### Physical Characteristics:

#### Width: 32 inches (81 centimeters).

#### Length: 32 inches (81 centimeters).

#### Height: 46 inches (117 centimeters).

#### Capacity: 44 gallons (167 liters).

#### Heavy-Duty Receptacle – Waste – HDRR55

#### Physical Characteristics:

#### Width: 32 inches (81 centimeters).

#### Length: 32 inches (81 centimeters).

#### Height: 52 inches (132 centimeters).

#### Capacity: 55 gallons (208 liters).

#### Heavy-Duty Receptacle – Waste – HDWR32

#### Physical Characteristics:

#### Width: 27 inches (69 centimeters).

#### Length: 27 inches (69 centimeters).

#### Height: 46 inches (117 centimeters).

#### Capacity: 32 gallons (121 liters).

#### Heavy-Duty Receptacle – Waste – HDWR44

#### Physical Characteristics:

#### Width: 32 inches (81 centimeters).

#### Length: 32 inches (81 centimeters).

#### Height: 46 inches (117 centimeters).

#### Capacity: 44 gallons (167 liters).

#### Heavy-Duty Receptacle – Waste – HDRR55

#### Physical Characteristics:

#### Width: 32 inches (81 centimeters).

#### Length: 32 inches (81 centimeters).

#### Height: 52 inches (132 centimeters).

#### Capacity: 55 gallons (208 liters).

## HEAVY DUTY CONDIMENT CABINETS

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SPECIFIER NOTES: DELETE PRODUCTS AND OPTIONS NOT REQUIRED FOR THIS PROJECT. OPTIONS WITHIN PRODUCTS ARE INDICATED BY SQUARE BRACKETS.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

### Heavy-Condiment Cabinets

#### Product Options:

#### Mix and Match Upgrade Custom Logo for Front or Sides: Contact the manufacturer for custom logo tops.

#### Heavy-Duty Condiment Cabinet HDCC2742

#### Physical Characteristics:

#### Depth: 27 inches (69 centimeters).

#### Width: 42 inches (107 centimeters).

#### Height: 50 inches (127 centimeters).

# EXECUTION

## INSTALLATION

### Do not install furnishing until the site has been properly prepared.

### Install furnishings in accordance with the manufacturer’s instructions and recommendations.

## ADJUSTMENT AND CLEANING

### Cleaning: Clean furnishings in accordance with the manufacturer’s instructions and recommendations.

## PROTECTION

### Protect installed products until completion of project.

### Touch-up, repair, or replace damaged products prior to Substantial Completion.

END OF SECTION